PP2178

0 up to 12 m

Al-Cast

appr. 18 x 75 x 33

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 70 mA without electrical load

bright-switching

PNP-Transistor, Optocoupler (alternatively)

LED (Switch Indicator, Working Indicator Transmitter)

- 25°C ... + 60°C

LB for Prevention of Accidents, cascadeable; self checking Control Unit PP2128ST or PP2129 ST neccessary; DIANA (Level Indicator)