PV2010/3

0 up to 50 m, with Tele 100 m

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 70 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/ Working-/ Pollution Warning Indicator)

- 25°C ... + 60°C

Cable Length between Transmitter and Receiver
up to 200 m;
Interference Suppression by Forced Synchronisation;
DIANA (Level Indicator);
Pollution Warning Output;
Steady light resistance >100kLx