JV191

0 up to 18 m with Reflektor G85

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 880 nm, visible

24 VDC / 60 mA without electrical load

bright- / dark- switching, selectable

PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/Pollution Warning Indicator)

- 30°C ... + 80°C

Time Delay 0-10s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator); Pollution Warning Output