PU2009/3

0 up to 120 m with Tele 200 m

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 80 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/ Working-/ Pollution Warning Indicator)

- 25°C ... + 60°C

Cable Length between Transmitter and Receiver up to 200 m; Interference Suppression by Forced Synchronisation; DIANA (Level Indicator); Intelligent Pollution Warning Output