ET192/800v

100 up to 1000 mm, adjustable

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 60 mA without electrical load

bright- / dark- switching, selectable

PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/Pollution Warning Indicator)

- 25°C ... + 60°C

active Background Response Suppression;
Pollution Warning;
Time Delay 0 up to 10 s,
switching-on-off-delay, separately adjustable;
Interference Suppression by Forced Synchronization;
DIANA (Level Indicator)