PP2441(q)/154/R27

0 up to 4 m

Al-Cast

appr. 57 x 175 x 80

IP 65

Plug and Socket Connection

LED 880 nm, invisible

mittels Steuergerät PP83201/2

bright- / dark- switching, selectable

Signal exchange between Transmitter and Receiver

LED (Switch-/ Working Indicator)

- 25°C ... + 60°C

Interference Suppression by Forced Synchronization; Application e.g.: Detection of hole marked welded seams; Operating width 154 mm