Light Grill Barrier PLG47...

0 up to 2 m

Al-Cast

appr. 250 x 80 x 58

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / ~600 mA without electrical load

bright- / dark- switching, selectable

PNP -Transistor

LED (Switch Indicator, in Receiver and Control Unit)

- 25°C ... + 60°C

Interference Suppression by Forced Synchronization; Resolution >5.5 mm; Operating width 56 mm; Other distance, resolution and operating widht on request.