JP171-1Ref

0 up to 2,5 m

Al-Cast

appr. 18 x 75 x 33

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 VDC / 40 mA without electrical load

bright- / dark- switching

PNP- / NPN-Transistor (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Forced Local Range; Glass Detection; reference value depending on object adjustable; Interference Suppression by Forced Synchronization