JU103/4

0.5 up to 35 m with Reflektor G85; up to 70 m with Reflektor GR50S

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible or Red Light 650 nm, visible

24 V DC / 60 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/Pollution Warning Indicator)

- 25°C ... + 60°C

Time Delay 0-10s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator); Intelligent Pollution Warning Output