PP24210-2

-

Al-Cast

appr. 260 x 160 x 90

IP 65

Terminal Block or Plug and Socket Connection

-

24 V DC / 60 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Control Unit with Pre-Amplifier for 4 Pairs of Optic Heads; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)