PP2198

0 up to 25 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 70 mA without electrical load

bright-switching

PNP-Transistor, Optocoupler (alternatively)

LED (Switch Indicator, Working Indicator Transmitter); DIANA (Level Indicator)

- 25°C ... + 60°C

LB for Prevention of Accidents, cascadeable; self checking Control Unit PP2128ST or PP2129ST neccessary