JP198-1

0 up to 5 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 VDC / 70 mA without electrical load

bright-switching

PNP-Transistor

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

LB for Prevention of Accidents, cascadeable;
self checking Control Unit PP2128ST or PP2129 ST neccessary;
Gloss suppression;
Forced Local Range;
Interference Suppression by Forced Synchronization;
DIANA (Level Indicator)