JP105RFZ.55

50 up to 600 mm, other distances upon request

Al-Cast

appr. 35 x 98 x 64

IP 65

Cable oder Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 60 mA without electrical load

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

passive Background Response Suppression; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)