JP172-1Ref

0 up to 2.5 m

Al-Cast

appr. 57 x 125 x 80

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 60 mA without electrical load

bright- / dark- switching, selectable

PNP- / NPN-Transistor (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Forced Local Range; Glass Detection; reference value depending on object adjustable; Interference Suppression by Forced Synchronization