PV1037/2*01

1 up to 25 m

Al-Cast

appr. 80 x 220 x 120

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

230 VAC / 10 VA; other voltages are possible

dark-switching

Relay, 2 x NC and 1 x NO, supervised and forceguided

2 LED's green (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Special Designs: external Test System; Sabotage Protection; Pollution Warning; Special design of PV1037/2: No scanning, distance reduced up to 25m