PP2004(N)

0 up to 200 m with Tele 400 m

Al-Cast

appr. 57 x 125 x 80

IP 66

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

230 VAC / 3 VA; other voltages are possible

bright- / dark- switching, changeable

Relay, NPN-Transistor, Optocoupler

LED (Switch-/ Working Indicator)

- 25°C ... + 60°C

Cable length between Transmitter and Receiver up to 200 m; Interference Suppression by Forced Synchronisation; DIANA (Level Indicator)