JP104RFZ.7

50 up to 700 mm

Al-Cast

appr. 57 x 125 x 80

IP 65

Cable oder Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 70 mA without electrical load

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Relay, Optocoupler (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

passive Background Response Suppression; Interference Suppression by Forced Synchronization