JP191-1Ref

0 up to 8 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 VDC / 40 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler, Relay (alternatively)

LED (Indicator) DIANA (Level Indicator)

- 25°C ... + 60°C

Forced Local Range; Detection of transparent objects; Interference Suppression by Forced Synchronization