EP192/800

100 up to 1000 mm, adjustable

Al-Cast

appr. 30 x 100 x 65

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 50 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

passive Background Response Suppression; Time Delay 0 up to 10 s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)