PP2441(q)/H/Al

0 up to 4 m

Al-Cast

appr. 70 x customized size x 110

IP 65

Plug and Socket Connection

LED 880 nm, invisible

from Control Unit PP83201/2

bright- / dark- switching, selectable

Signal exchange between Transmitter and Receiver

LED (Switch Indicator)

- 25°C ... + 60°C

Interference Suppression by Forced Synchronization; Application e.g.: Detection of hole marked welded seams; Operating width >308 mm