JP198d

0 up to 15 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 V DC / 70 mA without electrical load

dark-switching

PNP-Transistor

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

LB for Prevention of Accidents, cascadeable; self checking Control Unit PP2128ST or PP2129ST neccessary; Gloss suppression; Interference Suppression by Forced Synchronization