PV21112/2

-

Al-Cast

appr. 57 x 175 x 80

IP 65

Terminal Block or Plug and Socket Connection

-

24 VDC / 80 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

2 x: Relay, 2 x PNP / 2 x NPN - Transistor, Optocoupler (alternatively)

LED (Switch-/ Pollution Warning Indicator)

- 25°C ... + 60°C

Control Unit with Pre-Amplifier for 1 Pair of Optic Heads; Pollution Warning; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)