PV1038/2*04

1 up to 25 m

Al-Cast

appr. 91 x 260 x 160

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

230 VAC / 16 VA; other voltages are possible

dark-switching

2 x Relay, each 2 x NC and 1 x NO, supervised and forceguided

4 LED's green (Switch Indicator)

- 25°C ... + 60°C

Special Designs: external Test System; Sabotage Protection;
DIANA (Level Indicator);
Pollution Warning;
Special design of PP1038/2:
No scanning,
distance reduced up to 25m