JP103RFZ...PRFZ13

100 up to 1300 mm

Al-Cast

appr. 57 x 175 x 80

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 80 mA without electrical load

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Relay, Optocoupler (alternatively)

LED (Indicator); DIANA (Level Ind.)

- 25°C ... + 60°C

passive Background Response Suppression; Interference Suppression by Forced Synchronization