JV103RFZ...

100 up to 1300 mm

Al-Cast

appr. 57 x 175 x 80

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 60 mA without electrical load

bright- / dark- switching, selectable

PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/Pollution Warning Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

passive Background Response Suppression; Interference Suppression by Forced Synchronization; Pollution Warning Output