JP102/3

3 up to 50 m with Reflector G85; up to 140 m with Reflector GR50S

Al-Cast

appr. 57 x 175 x 162

IP 65

Term. Block or Plug and Socket Conn.

LED 880 nm, invisible

24 VDC / 50 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Time Delay 0-10s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization;