TRIV140210/L

100 up to 700 mm

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection

LED 650 nm, visible

24 V DC / 60 mA without electrical load

bright- / dark- switching, selectable

PNP-Transistor

LED (Switch-/Pollution Warning Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Reference Tuning with internal regulation screw; Pollution Warning; Interference Suppression by Forced Synchronization