JP104/3

0,5 up to 15 m with Reflector G85; up to 40 m with Reflector GR50S

Al-Cast

appr. 57 x 125 x 80

IP 65

Term. Block or Plug and Socket Conn.

LED 880 nm, inv. or Red Light 650 nm, v.

24 VDC / 50 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Time Delay 0-10s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)