PR1031RFZ

400 up to 1500 mm

Al-Cast

appr. 57 x 175 x 101

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 60 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

active Background Response Suppression; Interference Suppression by Forced Synchronization