PP2092/2

0 up to 80 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 70 mA without electrical load

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator/Working Indicator)

- 25°C ... + 60°C

Cable Length between Transmitter and Receiver up to 120 m; Interference Suppression by Forced Synchronisation; DIANA (Level Indicator)