JP191NTx

80 or 125 mm (alternatively

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 V DC / 60 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Time Delay 0 up to 10 s, ein- / ausschaltverzögernd, getrennt adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)