PU2092/2

0 up to 80 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 90 mA without electrical load

bright- / dark- switching, selectable

PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch-/ Working-/ Pollution Warning Indicator)

- 30°C ... + 80°C

Cable Length between Transmitter and Receiver up to 120 m; Interference Suppression by Forced Synchronisation; DIANA (Level Indicator); Intelligent Pollution Warning Output