PP26210-2

-

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection

-

24 VDC / 200 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP / NPN - Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Control Unit with Pre-Amplifier for 6 Pairs of Optic Heads; Interference Suppression by Forced Synchronization; DIANA (Level Indicator)