PP2005K

PP5522/2

Detectable Temperature > 500°C

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection; Fibre Optic Connection

-

24 VDC / 50 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler, Relay (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Use Optic Heads (Adapter) for long distances