PV1038/2

0.5 up to 45 m

Al-Cast

appr. 91 x 260 x 160

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

230 VAC / 16 VA; other voltages are possible

dark-switching

2 x Relay, each 2 x NC and 1 x NO, supervised and forceguided

4 LED's green (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Special Designs: external Test System; Sabotage Protection; Pollution Warning