PP5525/2*01

Detectable Temperature > 500°C

Al-Cast

appr. 57 x 125 x 103

IP 65

Terminal Block or Plug and Socket Connection

-

24 VDC / 50 mA without electrical load other voltages are possible

bright- / dark- switching, selectable

PNP- / NPN-Transistor, Optocoupler, Relay (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Single sided spreaded field of vision; Option: Input (Connection) for Test-Funktion