TRC1001

220 mm

Al-Cast

appr. 81 x 220 x 120

IP 65 /Optic Head IP 66

Terminal Block or Plug and Socket Connection; Fibre Optic Connection

LED's: 880/660/595 nm

24 VDC / 200 mA without electrical load

see Operating Manual

PNP- / NPN-Transistor, (alternatively)

LED's: Working Indicator, Operating Indicator, Error Indicator

- 10°C ... + 60°C Control Unit - 25°C ... + 200°C Optic Head

Application: Paper Break Detection