ET103/2000

300 up to 3000 mm, adjustable

Al-Cast

appr. 57 x 125 x 110

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 VDC / 40 mA without electrical load

bright- / dark- switching, selectable

PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 30°C ... + 65°C

Active Background Response Suppression; Time Delay 0 up to 10 s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization