JP193-1

JP193-1Ref

0 up to 5 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 VDC / 40 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 60°C

Forced Local Range; Detection of transparent objects; Gloss Suppression; Interference Suppression by Forced Synchronization