JV103/4GFK

5 m w/o Opti, 25 m w Optic Head

Al-Cast

appr. 57 x 125 x 80

IP 65

Terminal Block or Plug and Socket Connection; Fibre Optic Connection

LED 880 nm, invisible

24 VDC / 60 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler, Relay (alternatively)

LED (Switch-/Pollution Warning Indicator)

- 25°C ... + 60°C

Pollution Warning Output; DIANA (Level Indicator); Interference Suppression by Forced Synchronization