JP192-1

0 up to 10 m with Reflektor G85

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 880 nm, invisible

24 V DC / 60 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Time Delay 0-10s, switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator); Forced Local Range