JP705/XL

graded: 100 / 200 / 300 mm

Brass, Nickel plated

M 30 x 1,5 x 85

IP 65

Cable

LED 880 nm, invisible

24 VDC / 40 mA without electrical load

bright-switching

PNP- / NPN-Transistor (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

passive Background Response Suppression; Interference Suppression by Forced Synchronization; passive Background Response Suppression; DIANA (Level Indicator)