PV1037/2

0,5 up to 45 m

Al-Cast

appr. 80 x 220 x 120

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

230 VAC / 10 VA; other voltages are possible

dark-switching

Relay, je 2 x NC and 1 x NO, supervised and forceguided

2 LED's green (Switch Indicator); DIANA (Level Indicator)

- 25°C ... + 100°C

Special Designs: external Test System; Sabotage Protection; Pollution Warning