JP193

0 up to 15 m

Al-Cast

appr. 30 x 100 x 65

IP 65

Plug and Socket Connection

LED 650 nm, visible

24 VDC / 40 mA without electrical load; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 30°C ... + 80°C

Time Delay 0-10s,switching-on-off-delay, separately adjustable; Interference Suppression by Forced Synchronization; DIANA (Level Indicator); Gloss suppression