PP2441(q)/308/R153

0 up to 4 m

Al-Cast

appr. 120 x 360 x 80

IP 65

Terminal Block or Plug and Socket Connection

LED 880 nm, invisible

230 VAC / 10 VA; other voltages are possible

bright- / dark- switching, selectable

Relay, PNP- / NPN-Transistor, Optocoupler (alternatively)

LED (Switch Indicator)

- 25°C ... + 60°C

Interference Suppression by Forced Synchronization; Application e.g.: Detection of hole marked welded seams; Operating width 308 mm; Time Delay 0 bis 3 s