Reflex-Taster

| 1202 | ET103/2000 | adjustable scanning depth, active background response suppression, <3000mm
| 1202v | ET103/2000v | adjustable scanning depth, active background response suppression, unlinked pollution warning, <3000mm
| 1267 | JP192/800 | compact structural shape, passive background response suppression
| 1268 | ET192/800 | compact structural shape, adjustable scanning depth, active background response suppression, <1000mm
| 1268v | ET192/800v | compact structural shape, adjustable scanning depth, active background response suppression, unlinked pollution warning, <1000mm
| 1269 | EP192/800 | compact structural shape, adjustable scanning depth, passive background response suppression, <1000mm
| 1270 | JP705/xL | compact structural shape(M30), passive background response suppression, <300mm
| 1361 | JP191NTx | compact structural shape, passive background response suppression
| 1362 | JP192NTx | compact structural shape, passive background response suppression
| 1381 | JP171NT62 | extreme compact structural shape, passive background response suppression
| 1410 | JP105RFZ.2 | compact structural shape, high power, passive background response suppression
| 1420 | JP105RFZ.4 | compact structural shape, high power, passive background response suppression
| 1428 | JV105RFZ.4 | compact structural shape, high power, passive background response suppression, unlinked pollution warning
| 1430 | JP105RFZ.55 | compact structural shape, high power, passive background response suppression
| 1440 | JP104RFZ.7 | high power, passive background response suppression
| 1448 | JV104RFZ... | high power, passive background response suppression, unlinked pollution warning, <700mm
| 1450 | JP103RFZ... | high power, passive background response suppression, <1300mm
| 1458 | JV103RFZ... | high power, passive background response suppression, unlinked pollution warning, <1300mm
| 1452 | JP103RFZ...t | extreme high power, passive background response suppression, <3000mm
| 1459 | JV103RFZ...t | extreme high power, passive background response suppression, unlinked pollution warning, <3000mm
| 1456 | PR1031RFZ | high power, active background response suppression, <1500mm
| 1457 | PR1032RFZ | extreme high power, active background response suppression, <2800mm